# Updating the firmware

1. Save your changes.
2. Download the latest firmware file from the Weidmüller website.

1. On the Starting page, click Settings.
2. Click Firmware update.
4. Click Browse.
5. Choose the firmware file from your file system.
6. Click Open.
7. Click Start.
8. The upload is started.
9. u-create web is disconnected.
10. Node-RED flows are stopped.
11. SWupdate is displayed.
12. The device restarts.

1. u-create web is restarted.

Examine the software version in the About dialog to see whether the firmware update was successful.