# Temperature Controller for the Starter-Kit IoT

This example program shall ease the first setup of Weidmüller's [Starter-Kit IoT](https://www.weidmueller.com/int/service/support_for_u_control_starter_kits.jsp). It implements a simple temperature controller.
Please refer to the accompanying Quick Start Guide to setup your Starter-Kit. If you want to know more about this example application, take a look at the Application Note. Both are available for download at the URL above.


## Files  

 - qsg0033-starter-kit-iot-temperature-controller-v#.#.#.ucp  
   the u-create Web project containing the configuration for I/O-Modules, Global Variables and a u-create Visu Dashboard / HMI.
 - qsg0033-starter-kit-iot-temperature-controller-v#.#.#.json  
   The example Node-RED flow containing a simple temperature controller.
 - qsg0033-starter-kit-iot-temperature-controller-mqtt-v#.#.#.json  
   The extended example flow, implementing a MQTT publisher in addition to the temperature controller.
 - LICENSE  
   a copy of the MIT License
 - README.md  
   this file


## Copyright Notice

© 2021 Weidmüller Interface GmbH & Co. KG, Author: w100141
Published under the [MIT License](https://spdx.org/licenses/MIT.html).


## Changelog

 - v1.0.0 
   Initial release.
 - v1.0.1
   Minor cosmetic changes, naming for inputs and outputs of the function nodes.