# Updating the firmware

1. Save your changes.
2. Download the latest firmware file from the Weidmüller website.

1. On the Starting page, click Settings.
2. Click Firmware update.
3. SWUpdate is opened in a new browser tab.
5. Drag-and-drop the software update file into the dialogue box.
6. The upload is started.

1. When the upload is finished, the system is automatically restarted.

Examine the software version in the About dialogue to see whether the firmware update was successful.

Displaying the software version of u-create