# Configuring the Modbus TCP slave

A Modbus TCP slave can be configured to publish global variables defined in the real-time application via the Modbus TCP protocol.

The Modbus TCP slave is configured with a JSON file (see Editing a configuration file). If no configuration file is available on the device, you can download a configuration file template.

- Downloading a configuration file
- Editing a configuration file
- Loading a configuration file