# Checking manually for a firmware update via hawkBit client

You can check for a firmware update manually.

1. Prerequisite
2. You have connected the device to a hawkBit server.
3. You have set up your hawkBit server.

1. On the starting page, click Settings.
2. Click hawkBit settings.
3. Click Check for update.

1. The hawkBit client searches for a firmware update.
2. If a firmware update is available, it will be installed automatically.

Connecting the device to a hawkBit server