# Connecting the device to a hawkBit server

1. On the Starting page, click Settings.
2. Click hawkBit settings.
3. Enable the Enable hawkBit client check box.
4. In the URL text box, enter the URL and the port for the hawkBit server [example.com:8080].
5. If you want to use a target security token for authentication, enable the Use target security token check box and enter the target security token in the Target security token text box.
6. Edit the settings in your hawkBit server.
7. Click Apply.
8. Click Proceed to confirm.

What to do next

Set up your hawkBit server.